**Callflow for 5G Positioning Live Demo**

The following is the call flow used in the live demo. Note that 3GPP LPP Rel-16 (TS37.355) and NRPPa Rel-16 (TS38.455) can be used instead as the positioning protocols between the SLP and UE and between the SLP and MEC/gNB, respectively. Please also see OMA-TS-ULP-V2\_0\_6-20200720-D Section 5.2.1 for the SET-initiated SUPL call flow.

